general {
        colors = true
        interval = 5
}

order += "ethernet enp37s0"
order += "path_exists VPN"
order += "load"
order += "disk /"
order += "tztime local"
order += "tztime london"

ethernet enp37s0 {
        # if you use %speed, i3status requires the cap_net_admin capability
        format_up = "eth: %ip (%speed)"
        format_down = "eth"
}

battery all {
        format = "%status %percentage %remaining %consumption"
        format_down = "No battery"
	last_full_capacity = true
        status_chr = "⚡ CHR"
        status_bat = "🔋 BAT"
        status_unk = "? UNK"
        status_full = "☻ FULL"
        path = "/sys/class/power_supply/BAT%d/uevent"
        low_threshold = 20
}

run_watch DHCP {
        pidfile = "/var/run/dhclient*.pid"
}

run_watch VPNC {
        # file containing the PID of a vpnc process
        pidfile = "/var/run/vpnc/pid"
}

path_exists VPN {
        # path exists when a VPN tunnel launched by nmcli/nm-applet is active
        path = "/proc/sys/net/ipv4/conf/tun0"
}

tztime local {
        format = "Day: %d Local: %H:%M"
}

tztime london {
        format = "London: %H:%M"
        timezone = "Europe/London"
}

load {
        format = "%5min"
}

disk "/" {
        format = "%free"
}


